{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["GAPI Generator","Index parameters","Chart temp"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"GAPI Generator","index":0,"n_rows":34,"n_cols":2,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
[null,"GAPI chart generator"]
[]
[null,"• For detailed description refer to DOI: 10.1016/j.talanta.2018.01.013"]
[null,"• Please fill in the form using the drop-down lists"]
[null,"• You can copy the image and paste it anywhere you like"]
[]
[null,"Quantification"]
[null,"Select"]
[]
[null,"Sample preparation"]
[null,"Collection (1)"]
[null,"Preservation (2)"]
[null,"Transport (3)"]
[null,"Storage (4)"]
[null,"Type of method (5)"]
[null,"Scale of extraction (6)"]
[null,"Solvents / reagents used (7)"]
[null,"Additional treatments (8)"]
[]
[null,"Reagents and solvents"]
[null,"Amount (9)"]
[null,"Health hazard (10)"]
[null,"Safety hazard (11)"]
[]
[null,"Instrumentation"]
[null,"Energy (12)"]
[null,"Occupational hazard (13)"]
[null,"Waste (14)"]
[null,"Waste treatment (15)"]
[]
[]
[]
[null,"Wojciech Wojnowski 2018"]
[null,"wojciech.wojnowski@pg.edu.pl"]

{"sheet":"Index parameters","index":1,"n_rows":21,"n_cols":8,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
["Sample preparation"]
["Collection (1)","Preservation (2)","Transport (3)","Storage (4)","Type of method (5)","Scale of extraction (6)","Solvents / reagents used (7)","Additional treatments (8)"]
["In-line","None","None","None","No sample preparation","Nano-extraction","Solvent-free methods","None"]
["On-line or at-line","Chemical or physical","Required","Under normal conditions","Simple procedures","Micro-extraction","Green solvents / reagents","Simple treatments"]
["Off-line","Physico-chemical",null,"Under special conditions","Extraction required","Macro-extraction","Non-green solvents / reagents","Advanced treatments"]
[]
["Reagent and solvents"]
["Amount (9)","Health hazard (10)","Safety hazard (11)"]
["< 10 mL (< 10 g)","Slightly toxic, slight irritant; NFPA health hazard score of 0 or 1. No special hazards.","Highest NFPA flammability or instability score of 0 or 1. No special hazards."]
["10-100 mL (10-100 g)","Moderately toxic; could cause temporary incapacitation; NFPA = 2 or 3.","Highest NFPA flammability or instability score = 2 or 3, or a special hazard is used."]
["> 100 mL (> 100 g)","Serious injury on short-term exposure; known or suspected small animal carcinogen; NFPA = 4.","Highest NFPA flammability or instability score of 4."]
[]
["Instrumentation"]
["Energy (12)","Occupational hazard (13)","Waste (14)","Waste treatment (15)"]
["<= 0.1 kWh per sample","Hermetic sealing of the analytical process","< 1 mL (< 1 g)","Recycling"]
["<= 1.5 kWh per sample","Emission of vapours to the atmosphere","1-10 mL (1-10 g)","Degradation, passivation"]
["> 1.5 kWh per sample",null,"> 10 mL (>10 g)","No treatment"]
[]
["Select"]
["Procedure for qualification and quantification"]
["Procedure only for qualification"]

{"sheet":"Chart temp","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}